|  |
| --- |
| MICROCOM GPU v1.0 MANUAL |
|  |
| A hardware and software guide to using the Microcom GPU  10103  Authored by: J.Nock |



10103

Contents

[Technical Specifications 5](#_Toc66802190)

[Memory Map & Registers 6](#_Toc66802191)

[Memory map for EP4CE10 FPGA: 6](#_Toc66802192)

[Verilog HDL notes: 7](#_Toc66802193)

[MAGGIEs 8](#_Toc66802194)

[MAGGIE Registers 9](#_Toc66802195)

[BP2RAST\_cmd 10](#_Toc66802196)

[Bits 7-6 – Text\_mode\_master / text\_mode\_slave 10](#_Toc66802197)

[Bit 4 – mode\_565 10](#_Toc66802198)

[Bit 3 – BART enable 10](#_Toc66802199)

[Bit 2 – 16\_bit\_mode 10](#_Toc66802200)

[Bits 1-0 – Video Mode / pixels per byte 10](#_Toc66802201)

[Text Mode 11](#_Toc66802202)

[DEFAULT MAGGIE SETTINGS 12](#_Toc66802203)

[PALETTES 13](#_Toc66802204)

[ARGB4444 Palette 13](#_Toc66802205)

[Z80 Host IO ports 14](#_Toc66802206)

[Keyboard Interface 15](#_Toc66802207)

[KEYBOARD DATA PORT 15](#_Toc66802208)

[KEYBOARD STATUS REGISTER - READ 15](#_Toc66802209)

[PS/2 STATUS REGISTER – TYPEMATIC SETTINGS 16](#_Toc66802210)

[Hardware-Accelerated Graphics 18](#_Toc66802211)

[COMMAND/DATA WRITE ORDER 18](#_Toc66802212)

[HARDWARE COMMANDS 19](#_Toc66802213)

[X & Y registers 19](#_Toc66802214)

[Set destination screen memory pointer (7C-7F) 20](#_Toc66802215)

[Set source screen memory pointer (78-7B) 20](#_Toc66802216)

[Set destination raster width – X[2] (73) 20](#_Toc66802217)

[Set source raster width – X[2] (72) 21](#_Toc66802218)

[Set destination raster width – X[3] (71) 21](#_Toc66802219)

[Set source raster width – Y[3] (70) 21](#_Toc66802220)

[Set max width & height of screen – X[0]/Y[0] (5F) 22](#_Toc66802221)

[Set max width & height of screen – X[1]/Y[1] (5E) 22](#_Toc66802222)

[Set max width & height of screen – X[2]/Y[2] (5D) 22](#_Toc66802223)

[Set max width & height of screen – X[3]/Y[3] (5C) 23](#_Toc66802224)

[Clear pixel collision counter (5B) 23](#_Toc66802225)

[Clear blitter copy pixel collision counter (5A) 23](#_Toc66802226)

[Graphics Commands 24](#_Toc66802227)

[VWAIT – 0x07 25](#_Toc66802228)

[SET HW\_POSITION – 0x0F 25](#_Toc66802229)

[Blitter 27](#_Toc66802230)

[Blitter Copy Width & Height – X[2]/Y[2] & X[3]/Y[3] (74-75) 27](#_Toc66802231)

[Blitter Source Image Offset – X[2]/Y[2] & X[3]/Y[3] (76-77) 27](#_Toc66802232)

[Blitter Copy Source Pointer – X/Y[0-3] (78-7B) 28](#_Toc66802233)

[Blitter Copy Destination Pointer – X/Y[0-3] (7C-7F) 28](#_Toc66802234)

[Source/Destination X/Y Scaling (09) 28](#_Toc66802235)

[How to calculate a zoom 29](#_Toc66802236)

[Copy Colour Transform (08) 30](#_Toc66802237)

[Blitter Function – (00) 31](#_Toc66802238)

[HAG Bit Plane Values 31](#_Toc66802239)

[Appendix A – Character Codepage 32](#_Toc66802240)

|  |
| --- |
| Technical Specifications Depending on the FPGA used in the uCOM GPU card, the following features will be available in varying capacities. Listed below are *minimum specifications* based on an Intel EP4CE6 FPGA (used in initial development of the prototype GPU):   * 22KB FPGA graphics RAM, plus 1 KB for palettes * Up to 7 graphics layers * 320x240 resolution in 4 colours (19.2KB) at 60 fps (VGA) * Various palettes from 4,096 colours   A Cyclone IV EP4CE10 FPGA (used in the first proper video card) provides the following:   * 40KB FPGA graphics RAM, plus 1 KB for palettes * Up to 10 graphics layers * Audio buzzer * 640x480 resolution in 2 colours (38.4KB) at 60 fps (VGA)   A Cyclone V 5CEBA2 FPGA (2nd-generation video card) provides the following:   * 170KB FPGA graphics RAM, plus 1 KB for palettes * 16MB scratchpad RAM * Up to 20 graphics layers * 24-bit audio * 640x480 resolution in 16 colours (153.6KB) at 60 fps (VGA & DVI-D/HDMI) * 24-bit true-colour output   **NOTE:** *All 16-bit words in the uCOM GPU are big-endian*. |
|  |

|  |
| --- |
| Memory Map & Registers The uCOM GPU uses a vacant 512 KB slot in the host system’s memory space – see the uCOM’s manual for more information on this. This 512 KB window is filled with the GPU’s own RAM – if the GPU has less than 512 KB of RAM, accessing memory above the GPU’s upper memory limit will return FF values and be read-only (writes will be ignored).  *Only the last 16 bytes of the last page of the 512KB will return anything other than FF, and this will be the BANK\_ID as per the uCOM’s memory specifications. This is a pseudo-ROM location, with a value returned from a hardwired value in the HDL of the FPGA.*  For GPUs with access to scratchpad RAM, this will be presented as paged-RAM within the uCOM’s 512KB memory window, controlled via IO writes/reads to the GPU Memory Controller. Memory map for EP4CE10 FPGA:  * 0000-01FF – GPU HW registers:   + **00-07** = H&V triggers for 4 yellow test cursors   + **0C-0D** = H&V reset coordinates for all 15 MAGGIE\_Layer#s   + **10-13 + 4\*MAGGIE\_Layer#** = H&V top left edge of each MAGGIE\_Layer# window   + **60 + 10\*MAGGIE\_Layer#** = 16 byte controls for each of the 15 MAGGIE layers * 0200-11FF – Default IBM VGA 8x16 font. * 1200-9FFF – Video RAM (for text buffers / sprite data)   + **1200-1B5F** – Typical memory space for a full screen of text * A000-A3FF – Palettes:   + **A000-A1FF** – primary palette (ARGB4444)   + **A200-A3FF** – secondary palette (RGB565)   Without text you can mix 10 on-screen sprites, or 1 text layer and 8 sprites. Other than a RAM limitation, there are no other output limitations. Any mode and any resolution with any palette may all be mixed simultaneously onscreen. Verilog HDL notes: NUM\_LAYERS = 2 through 15 = 2 layers through 15 layers.  PALETTE\_ADDR = Sets the base address for the 2 palettes.  Palettes occupy the last 1024 bytes of GPU RAM. If the RAM ends on 2^ADDR\_SIZE (i.e. 32768), then (2\*\*ADDR\_SIZE)-1024 can be used to set PALETTE\_ADDR, otherwise PALETTE\_ADDR must be set explicitly to the last 1KB of available GPU RAM. Obviously, this depends on the amount of RAM available in the FPGA used. |
| MAGGIEs The **M**ultiple **A**ddress **G**enerator and **G**raphic **I**nstruction **E**ngines are the workhorses of the GPU. There are 10 MAGGIEs in the smallest system, numbered 0-9.  All MAGGIEs have their HV resets set to HV\_Trigger 0C & 0D.  MAGGIE top-left window X/Y positions:   * MAGGIE0 at HV\_Trigger 0010-11 & 0012-13 * MAGGIE1 at HV\_Trigger 0014-15 & 0016-17 * MAGGIE2 at HV\_Trigger 0018-19 & 001A-1B * MAGGIE3 at HV\_Trigger 001C-1D & 001E-1F * MAGGIE4 at HV\_Trigger 0020-21 & 0022-23 * MAGGIE5 at HV\_Trigger 0024-25 & 0026-27 * MAGGIE6 at HV\_Trigger 0028-29 & 002A-2B * MAGGIE7 at HV\_Trigger 002C-2D & 002E-2F * MAGGIE8 at HV\_Trigger 0030-31 & 0032-33 * MAGGIE9 at HV\_Trigger 0034-35 & 0036-37   MAGGIE register addresses – 16 bytes for each MAGGIE:   * Maggie Simpson - WikipediaMAGGIE0 – 0060 * MAGGIE1 – 0070 * MAGGIE2 – 0080 * MAGGIE3 – 0090 * MAGGIE4 – 00A0 * MAGGIE5 – 00B0 * MAGGIE6 – 00C0 * MAGGIE7 – 00D0 * MAGGIE8 – 00E0 * MAGGIE9 – 00F0 |

## MAGGIE Registers

|  |  |  |
| --- | --- | --- |
| Address | Name | Function |
| Base + 00 | BP2RAST\_cmd | Video Mode setting. *See page 10.* |
| Base + 01 | BP2RAST\_bgc | Background colour. |
| Base + 02 | BP2RAST\_fgc | Foreground colour. |
| Base + 03 | RST\_ADDR\_H | MSB bits of 24-bit base read address. |
| Base + 04 | RST\_ADDR\_M | MID bits of 24-bit base read address. |
| Base + 05 | RST\_ADDR\_L | LSB bits of 24-bit base read address. |
| Base + 06 | YINC\_ADDR\_H | MSB of bytes per line (*varies with video mode*) |
| Base + 07 | YINC\_ADDR\_L | LSB of bytes per line (*varies with video mode*) |
| Base + 08 | X\_SIZE\_H | MSB of display width in pixels. |
| Base + 09 | X\_SIZE\_L | LSB of display width in pixels. |
| Base + 0A | Y\_SIZE\_H | MSB of display height screen lines. |
| Base + 0B | Y\_SIZE\_L | LSB of display height screen lines. |
| Base + 0C | X\_SCALE | Two 4-bit nybbles. Upper 4 bits control X-increment every period, lower 4 is pixel period counter to define number of pixels until upper 4 bits are added to the address pointer. |
| Base + 0D | Y\_SCALE | Two 4-bit nybbles. Upper 4 bits reserved for text tile mode Y-size; lower 4 bits is line period counter to define number of lines until YINC\_ADDR is added to address pointer. |
| Base + 0E | X\_START\_SUB | 8-bit word. Defines an odd pixel start position within the period counter and X-position within a bit plane’s X-coordinate position. |
| Base + 0F | Y\_START\_SUB | 8-bit word. Defines an odd line start within the period counter and Y-coordinates inside a font. |

### BP2RAST\_cmd

The BP2RAST\_cmd register is composed of the following bit settings:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0 |
| text\_mode\_master | text\_mode\_slave | not used | mode\_565 | bart\_enable | 16\_bit\_mode | Video Mode | Video Mode |

#### Bits 7-6 – Text\_mode\_master / text\_mode\_slave

When using text/font/tile mode, two adjacent MAGGIEs must be used. The first one must have the '*text\_mode\_master*' bit set in the '*BP2RAST\_cmd*' while the second MAGGIE must have the '*text\_mode\_slave*' bit set in the '*BP2RAST\_cmd*'. These bits must be zero for non-tiled raw graphics modes.

#### Bit 4 – mode\_565

#### Bit 3 – BART enable

This bit must be HIGH for the linked BART to output pixel data. If the bit is LOW, the MAGGIE/BART pipeline is effectively turned off, unless the MAGGIE is a text\_mode\_master.

#### Bit 2 – 16\_bit\_mode

If HIGH, the BART works in 16-bit mode (so all addresses must be even) to use two-byte words when reading the pixel data.

#### Bits 1-0 – Video Mode / pixels per byte

Determines the Video Mode, or pixels per byte. The table below shows how bits 2-0 work together to determine the Video Mode:

|  |  |  |  |
| --- | --- | --- | --- |
| Bit 2 | Bit 1 | Bit 0 | Video Mode |
| 0 | 0 | 0 | 1-bit colour |
| 0 | 0 | 1 | 2-bit colour |
| 0 | 1 | 0 | 4-bit colour |
| 0 | 1 | 1 | 8-bit colour |
| 1 | 0 | 0 | 16-bit, 8 pixels-per-word |
| 1 | 0 | 1 | 16-bit, 4 pixels-per-word |
| 1 | 1 | 0 | 16-bit, 2 pixels-per-word |
| 1 | 1 | 1 | 16-bit, true colour |

## Text Mode

Two MAGGIEs are required for text mode – a master and a slave – and they must be neighbouring units (i.e. MAGGIE0 & MAGGIE1, MAGGIE3 & MAGGIE4 etc). The master MAGGIE positions the window on the screen and points to the source data (*screen buffer*), the slave MAGGIE sets foreground and background colours. The screen buffer location is specified in the master MAGGIE in the 24-bit word at register addresses +3 to +5. The Video Mode in both MAGGIEs must match, except in the master where the BP2RAST\_cmd BART\_enable (bit 3) must be disabled; otherwise you will get junk on the screen.

In 16-bit text mode, each character tile is followed by a palette byte. The upper 4-bits control the foreground colour, the lower 4-bits control the background colour. All other controls are the same as when using it as a bitmap graphics window.

The '*font\_y\_size*', combined upper bits of '{hw\_regs[Y\_START\_SUB][7:6], hw\_regs[Y\_SCALE][7:4]}' in the *text\_mode\_master* which must also be set to the font/tile height -1 (e.g.: 0=1 line, 7=8 lines, 15=16 lines, 31=32 lines) when in text/font/tile master mode.

For the *'text\_mode\_slave*' MAGGIE, the only functioning 4 controls are:

1. reset\_addr which points to the base memory address for font/tile graphics data,
2. period\_x[4] which defines a font as 16 pixels wide when set, or 8 pixels when low, and period\_x[3:0] which mask out the upper bits for fonts/tile addressing for 256, 512, 1024, 2048, 4096 characters (used in 16 bit addressing mode, otherwise set these bits to 0),
3. period\_y[1:0] which defines the font height (0=8, 1=16, 2=32, 3=64 lines tall), and
4. BP2RAST\_cmd which should match the *text\_mode\_master* MAGGIE settings except for the master and slave bit.

All base memory address settings should be on an even byte when using 16-bit mode. Fonts/tile graphics data should always begin on an even byte address.

## DEFAULT MAGGIE SETTINGS

Example default MAGGIE settings for the ‘chip’ image:

Top image: MAGGIE4 - HW triggers @ 20-21 & 22-23

A0 - 1A 10 00 00 33 00 00 60 00 BF 00 77 00 00 00 00

Middle image: MAGGIE5 - HW triggers @ 24-25 & 26-27

B0 - 1A 70 00 00 33 00 00 60 00 BF 00 77 01 01 00 00

Background image: MAGGIE6 - HW triggers @ 28-29 & 2A-2B

C0 - 0A B0 00 00 33 0A 00 60 00 BF 00 77 03 03 00 00

# PALETTES

The palettes are held in memory at $A000-$A3FF and are 512 entries wide, with the 4444 colour palette occupying the first 256x16 entries while the 565 palette occupies the second 256x16 entries. Both palettes are 16-bit.

## ARGB4444 Palette

This is the default palette for Text Mode, requiring two bytes per palette entry. As it is commonly used with Text Mode, which can specify a maximum of 16 index values, it is generally divided into separate palettes of 16 entries, with the first 16 being the default palette.

Each entry consists of two bytes, as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| 1st BYTE | | 2nd BYTE | |
| 4-bits | 4-bits | 4-bits | 4-bits |
| Transparency | RED | GREEN | BLUE |

*uCOM note:*

*Four pages of Bank 0x42 contains the palette, with the first 32 bytes containing the default palette. If Bank 0x42 is mapped to Area 3, the palette memory starts at 0xE000 and ends at 0xE3FF.*

# Z80 Host IO ports

The Z80\_Bridge in the GPU exposes some specific IO addresses to the host to facilitate extra hardware functions, listed below. The IO addresses are separate from the GPU RAM address space and are easily customizable in Quartus via the parameter settings in the Z80\_bridge.

|  |  |  |  |
| --- | --- | --- | --- |
| **IO Address** | **Read/Write** | **Function** | More on page |
| **240 / F0** | Read-only | KEYBOARD DATA port (*keyboard interface*) | 15 |
| **241 / F1** | Read/Write | KEYBOARD STATUS register (*keyboard interface*) | 15 |
| **242 / F2** | Write-only | SPEAKER ENABLE (0 = off, >0 = on) |  |
| **243 / F3** | Write-only | VIDEO OUTPUT ENABLE (0 = off, >0 = on) |  |
| **244 / F4** | Write-only | TONE (frequency) REGISTER for speaker (0-255) |  |
| **245 / F5** | Write-only | DURATION REGISTER for speaker (0-255) |  |
| **246 / F6** | Write-only | HAG LBR – Low-Byte Register (0-255) | 17 |
| **247 / F7** | Write-only | HAG HBR – High-Byte Register (0-255) | 17 |
| **248 / F8** | Read-only | HAG FIFO Status (FIFO full on bit 0) |  |

# Keyboard PS/2 Interface

The uCOM GPU provides far more than just a video output terminal. The GPU card also provides a keyboard terminal to fully release the uCOM from its dependency on a serial link to a host PC.

## KEYBOARD DATA PORT

This 8-bit data port returns the ASCII character with current MAKE or BREAK code (bit 7 set for BREAK, cleared for MAKE). ASCII characters are returned as a result of a key being pressed on the keyboard attached to the GPU card. Once read, the KEYBOARD DATA PORT is set to zero – any further reads will return 0x00 unless another MAKE or BREAK code is ready to be transmitted.

## KEYBOARD STATUS REGISTER - READ

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0 |
| TX | TX ACK | TX ERR | SHIFT | CAPS | EXT CODE | BREAK | VALID\_DATA |

When read, the KEYBOARD STATUS register provides information on the current state of the KEYBOARD DATA PORT and attached keyboard:

* Bit 0 – HIGH if valid data is available on the DATA port.
* Bit 1 – HIGH if the ASCII character at the DATA port is a BREAK code (i.e. the result of the key being released on the keyboard). *BREAK codes are generally filtered out by the DMI and CP/M BIOS (unless special code is written to make use of them) by ignoring characters with bit 7 set, or status bytes with bit 1 set.*
* Bit 2 – HIGH if the data is an EXTENDED CODE – another byte should be incoming.
* Bit 3 – HIGH if CAPS LOCK is active.
* Bit 4 – HIGH if SHIFT is depressed.
* Bit 5 – HIGH if no TX ACK received from keyboard in response to a command sent to it.
* Bit 6 – HIGH for TX acknowledge from keyboard
* Bit 7 – HIGH whilst data is transmitted to the keyboard

## KEYBOARD STATUS REGISTER – TYPEMATIC SETTINGS

Writing to the KEYBOARD STATUS register will set the keyboard’s *Typematic Delay* and *Repeat Rate*. In this way, the keyboard’s behaviour can be customized by the user as desired by simply writing a byte to the appropriate I/O address.

The delay and repeat rate are set in the same byte, which his composed as below:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0 |
| 0 | Delay | | Repeat Rate | | | | |

|  |  |
| --- | --- |
| Bits 5-6 | Delay (seconds) |
| 00b (00h) | 0.25 |
| 01b (20h) | 0.50 |
| 10b (40h) | 0.75 |
| 11b (60h) | 1.00 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Bits 0-4 | Rate (cps) | Bits 0-4 | Rate (cps) | Bits 0-4 | Rate (cps) | Bits 0-4 | Rate (cps) |
| 00h | 30.0 | 08h | 15.0 | 10h | 7.5 | 18h | 3.7 |
| 01h | 26.7 | 09h | 13.3 | 11h | 6.7 | 19h | 3.3 |
| 02h | 24.0 | 0Ah | 12.0 | 12h | 6.0 | 1Ah | 3.0 |
| 03h | 21.8 | 0Bh | 10.9 | 13h | 5.5 | 1Bh | 2.7 |
| 04h | 20.7 | 0Ch | 10.0 | 14h | 5.0 | 1Ch | 2.5 |
| 05h | 18.5 | 0Dh | 9.2 | 15h | 4.6 | 1Dh | 2.3 |
| 06h | 17.1 | 0Eh | 8.6 | 16h | 4.3 | 1Eh | 2.1 |
| 07h | 16.0 | 0Fh | 8.0 | 17h | 4.0 | 1Fh | 2.0 |

To work out a byte value to write to the register, simply add the hexadecimal values of your chosen settings together from the tables above. For example, if you want a delay of 0.50 seconds and a repeat rate of 10.0, add 20h and 0Ch together to get 2Ch. Write this byte to the PS/2 STATUS register and off you go.

NOTE: Valid values range from 00h-7Fh. Bit 7 should always be zero.

# Hardware-Accelerated Graphics

The HAG engine is a powerful hardware module in the GPU that performs basic graphics functions on behalf of the host system – including:

1. Pixel plotting (X[0], Y[0])
2. Line drawing (X[0], Y[0] to X[1], Y[1])
3. Filled/unfilled rectangle (X[0], Y[0] to X[1], Y[1])
4. Filled/unfilled triangle (X/Y[0], X/Y[1], X/Y[2])
5. Filled/unfilled quadrilaterals (X/Y points [0] to [3])
6. Blitter copy/paste with rotation & scaling

As well as the primary drawing functions, there are several support functions:

* Set 24-bit destination screen memory pointer
* Set 24-bit source screen memory pointer
* Set byte-width for destination raster (in x[n], y[n]) (n = 2 to 3)
* Set byte-width for source raster (in x[n], y[n]) (n = 2 to 3)
* Set maximum bitmap width & height to x[n], y[n] (n = 0 to 3)
* Clear pixel collision counter
* Clear blitter copy pixel collision counter

## COMMAND/DATA WRITE ORDER

The HAG has a 16-bit interface, driven by multiple IO writes from the host in little-endian format – the LOW byte is always written first to IO port 246, then the HIGH byte – which causes the GPU to act on the received 16-bit data/command – is written to IO port 247. Data/commands should be written in pairs – even if a value of zero is required for a command, the low byte should have zero written to it before writing to the High-Byte Register. This ensures the Low-Byte Register does not insert garbage values into the code.

## HARDWARE COMMANDS

### X & Y registers

There are four 12-bit X and Y registers, X[0-3], Y[0-3]. Their contents are set using the 16-bit input (HAG LBR and HBR) register. As with all data sent to the HAG, the low byte must be written first to port 246, followed by the high byte to port 247.

NOTE: The command bytes (sent to the High-Byte Register) may also include data in their lower nybble.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE (HBR) | | | | | | | | LOW BYTE (LBR) | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 1 | R | n | n | ? | ? | ? | ? | ? | ? | ? | ? | ? | ? | ? | ? |


R – HBR bit 6 (register bit 14) – Register Select

This bit determines which register – X or Y – is being written to. 0 = X, 1 = Y.

nn – HBR bits 5 & 4 (register bits 13 & 12)

These bits specify which of the four X/Y registers to write to.

? – bits 0-11 are 12 data bits to be written to the specified register. Room for three nybbles (or three hex digits). Note that 4 bits in the HBR (green boxes) can also be used to include data, e.g., when setting a base memory address.

In the example below, a base address of ABCDE is set by writing 0x0AB to Y[3] with the F0AB command word, and 0xCDE to X[3] with the BCDE command word.

### Set destination screen memory pointer (7C-7F)

The following command sets the destination screen memory pointer to the data in the indicated 12-bit registers. LBR value is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 1 | 1 | n | n | x | x | x | x | x | x | x | x |

* nn – specify which of the four X/Y registers to use the data from
* x – don’t care – these bits are ignored

### Set source screen memory pointer (78-7B)

The following command sets the source screen memory pointer to the data in the indicated 12-bit registers. LBR value is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 1 | 0 | n | n | x | x | x | x | x | x | x | x |

* nn – specify which of the four X/Y registers to use the data from
* x – don’t care – these bits are ignored

### Set destination raster width – X[2] (73)

Sets the destination raster’s bytes-per-horizontal line to the data in the X[2] register. Y register is ignored. Low byte bits 2-0 specify bits-per-pixel.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 0 | 1 | 1 | x | x | x | x | x | bpp | | |

* x – don’t care – these bits are ignored
* bpp – bits per pixel

### Set source raster width – X[2] (72)

Sets the source raster’s pixels-per-horizontal line to the data in the X[2] register. Y register is ignored. Low byte bits 2-0 specify bits-per-pixel.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 0 | 1 | 0 | x | x | x | x | x | bpp | | |

* x – don’t care – these bits are ignored
* bpp – bits per pixel

### Set destination raster width – X[3] (71)

Sets the source raster’s pixels-per-horizontal line to the data in the X[3] register. Y register is ignored. Low byte bits 2-0 specify bits-per-pixel.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 0 | 0 | 1 | x | x | x | x | x | bpp | | |

* x – don’t care – these bits are ignored
* bpp – bits per pixel

### Set source raster width – Y[3] (70)

Sets the source raster’s bytes-per-horizontal line to the data in the Y[3] register. X register is ignored. Low byte bits 2-0 specify bits-per-pixel.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 0 | 0 | 0 | x | x | x | x | x | bpp | | |

* x – don’t care – these bits are ignored
* bpp – bits per pixel

### Set max width & height of screen – X[0]/Y[0] (5F)

Sets the bitmap dimensions to the data in the 0-index registers (X[0], Y[0]). LBR value is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 0 | 1 | 1 | 1 | 1 | 1 | x | x | x | x | x | x | x | x |

x – don’t care – these bits are ignored.

### Set max width & height of screen – X[1]/Y[1] (5E)

Sets the bitmap dimensions to the data in the 1-index registers (X[1], Y[1]). LBR value is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | x | x | x | x | x | x | x | x |

x – don’t care – these bits are ignored.

### Set max width & height of screen – X[2]/Y[2] (5D)

Sets the bitmap dimensions to the data in the 0-index registers (X[0], Y[0]). LBR value is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 0 | 1 | 1 | 1 | 0 | 1 | x | x | x | x | x | x | x | x |

x – don’t care – these bits are ignored.

### Set max width & height of screen – X[3]/Y[3] (5C)

Sets the bitmap dimensions to the data in the 3-index registers (X[3], Y[3]). LBR value is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 0 | 1 | 1 | 1 | 0 | 0 | x | x | x | x | x | x | x | x |

x – don’t care – these bits are ignored.

### Clear pixel collision counter (5B)

Clears the pixel collision counter and sets all three transparent mask colours to one 8-bit colour in the source function data.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 0 | 1 | 1 | 0 | 1 | 1 | ? | ? | ? | ? | ? | ? | ? | ? |

? – sets the mask colour.

### Clear blitter copy pixel collision counter (5A)

Clears the blitter copy pixel collision counter and sets all three transparent mask colours to one 8-bit colour in the source function data.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 0 | 1 | 1 | 0 | 1 | 1 | ? | ? | ? | ? | ? | ? | ? | ? |

? – sets the mask colour.

# Graphics Commands

Following is a summary of the graphics commands that can be sent to the GPU using the hardware commands listed previously via IO calls, or whatever interface your system uses. All commands are 16-bit, with the low byte sent first.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| # | Command | High Byte | Low Byte | Notes |
| 1 | Draw Pixel | 01 | Colour | Draws a pixel at X/Y[0]. |
| 2 | Draw Line | 02 | Colour | Draws a line from X/Y[0] to X/Y[1]. |
| 3 | Draw Triangle | 03 | Colour | Draws a triangle with points X/Y[0], [1] and [2]. |
| 4 | Draw Rectangle | 04 | Colour | Draws a rectangle, top-left corner at X/Y[0], bottom-right corner at X/Y[1]. |
| 5 | Draw Quad | 05 | Colour | Draws a quad, corners specified using all four X/Y registers. |
| 6 | Draw Arc | 06 | Colour | Draws an arc (quarter of an ellipse based on quadrant # set in next command). Uses X/Y[0] for centre, X/Y[1] to set X & Y radii. To draw a complete ellipse or circle, this must be executed four times, once for each quadrant. |
| 7 | Quadrant Select | 07 | 0x00-0x03 | Set the ellipse quadrant to draw. This must be set before Draw Arc is executed. To draw a complete ellipse or circle, this must be executed four times, once for each quadrant. |
| 7 | VWAIT | 07 | 0x8#-0xB#  (# = 1-F) | 0x8# .. 0x8# => Wait for hw\_position\*1 to pass by # frames.  0x9# .. 0x9# => Wait for hw\_position\*2 to pass by # frames.  0xA# .. 0xA# => Wait for hw\_position\*4 to pass by # frames.  0xB# .. 0xB# => Wait for hw\_position\*8 to pass by # frames. |
| … |  |  |  |  |
| 11 | Filled Triangle | 0B | Colour | Draws filled triangle, points at X/Y[0], [1] and [2]. |
| 12 | Filled Rectangle | 0C | Colour | Draws filled rectangle, top-left corner at X/Y[0], bottom-right corner at X/Y[1]. |
| 13 | Filled Quad1 | 0B  0D | Colour  Colour | Drawing a quad utilises the Filled Triangle command and the alternative Filled Triangle command that uses points from registers 0, 2 and 3. Point order must be clockwise. |
| 14 | Filled Arc | 0E | Colour | As Draw Arc, except filled. |
| 15 | Set hw\_position | 0F | hw\_position | Used with VWAIT. Default 0. |

1 – This hybrid command requires two sets of 16-bit commands to be sent to the IO port

## VWAIT – 0x07

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 | 0 | Multiplier | | Multiplicand | | | |

The VWAIT command tells the GPU to wait a specified time (using a multiple of the *hw\_position* value) before executing the next instruction. *VWAIT shares the same command High Byte as Quadrant Select; Low Byte values 0x00-0x03 are strictly reserved for Quadrant Select, valid range for VWAIT’s Low Byte is 0x81-0xBF.*

The multiplier is set by bits 5 and 4 in the Low Byte of the command to x1, x2, x4 or x8 – with the multiplicand being the least-significant nybble (valid range: 0x01-0x0F).

|  |  |  |
| --- | --- | --- |
| **Multiplier** | **Multiplicand** |  |
| **0x8** | 0x81-0x8F | Wait for (*hw\_position* x 1) to pass by # frames. |
| **0x9** | 0x91-0x9F | Wait for (*hw\_position* x 2) to pass by # frames. |
| **0xA** | 0xA1-0xAF | Wait for (*hw\_position* x 4) to pass by # frames. |
| **0xB** | 0xB1-0xBF | Wait for (*hw\_position* x 8) to pass by # frames. |

## SET HW\_POSITION – 0x0F

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | hw\_position | | | | | | | |

Sets the *hw\_position* value used with the VWAIT command.

*hw\_position* defaults to zero, unless set to another value using this command. A value of zero means the vertical wait position is one line after the display frame has ended, giving the maximum time before the next frame begins to draw.

To request a delay before executing the next command, the multiplicand set with the VWAIT command needs to be 1 or higher to wait multiple frames. A *hw\_position* of 100 and using VWAIT with a Low Byte value of 0xA1 means the pause position will be located 400 line/h-syncs after the end of the display frame.

Values of *hw\_position* larger than the available lines in the frame will cause VWAIT to abort after a 2-frame pause.

# Mosaic,grid,pixel,pattern,decoration - free image from needpix.comBlitter

The HAG has a fully functional blitter to massively speed up sprite operations (block copy & paste). *All draw commands will blit.* If you use command '0x01' (plot pixel), the paste will begin at coordinates X/Y[0], or be center-shifted depending on set width & height when ‘Center Paste’ is enabled (see page 25). If you use the line command '0x02', the blitter will paste a new copy of the source image for every single pixel in the source line coordinates X/Y[0] - X/Y[1], using the source image like a brush.

### Blitter Copy Width & Height – X[2]/Y[2] & X[3]/Y[3] (74-75)

Sets the bitmap dimensions to copy – width is set by the X register contents, height by Y. Bit 0 in the High Byte specifies which register set to use (2/3). Each dimension has 1 added (e.g. X[2] = 0 would give a width of 1). Low byte is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 1 | 0 | n | x | x | x | x | x | x | x | x |

* n – specifies which register set (low = X/Y[2], high = X/Y[3])
* x – don’t care – these bits are ignored

### Blitter Source Image Offset – X[2]/Y[2] & X[3]/Y[3] (76-77)

Sets the source image (copy/read) offset. Bit 0 in the High Byte specifies which register set to use (2/3). Low byte is ignored.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 1 | 1 | n | x | x | x | x | x | x | x | x |

* n – specifies which register set (low = X/Y[2], high = X/Y[3])
* x – don’t care – these bits are ignored

### Blitter Copy Source Pointer – X/Y[0-3] (78-7B)

Sets the blitter memory source pointer – using the 12-bit Y (MSW) and X (LSW) register contents. Bits 0-1 in the High Byte specifies which register set to use (0-3). Low byte in the command word specifies the source *screen mode*, or bits per pixel.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 1 | n | n | Screen\_mode (bpp)  x  x  x  x  x  x  x | | | | | | | |

* nn – specifies which register set (X/Y[0-3])

### Blitter Copy Destination Pointer – X/Y[0-3] (7C-7F)

Sets the blitter memory destination pointer – using the 12-bit Y (MSW) and X (LSW) register contents. Bits 0-1 in the High Byte specifies which register set to use (0-3). Low byte in the command word specifies the destination *screen mode*, or bits per pixel.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 1 | 1 | 1 | 0 | 1 | n | n | Screen\_mode (bpp)  x  x  x  x  x  x  x | | | | | | | |

* nn – specifies which register set (X/Y[0-3])

### Source/Destination X/Y Scaling (09)

Sets the blitter’s scaling function, enabling up- and down-scaling of bitmaps during copy/pasting or disabling scaling altogether.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 0 | 0 | 0 | 1 | 0 | 0 | 1 | x | x | x | x | x | x | f | f |

* f – specifies scaling option (see table below)
* x – don’t care – these bits are ignored

Bits 0 & 1 of the Low Byte specify the scaling features as per the table below:

|  |  |  |
| --- | --- | --- |
| **Bit** | **Function** | **Details** |
| 0 | Up-scaling | HIGH – Enables blitter up-scaling of the source image, specified by registers X[0] and Y[0] for width & height accordingly. |
| 1 | Down-scaling | HIGH – Enables blitter down-scaling of the pasted image, specified by registers X[1] and Y[1] for width & height accordingly. |

**How to calculate a zoom**

Valid scale factor settings range from 1-4096. Values outside this range will default the setting back to 4096.

To enlarge the source bitmap, set the down-scaling to 4096 (1:1, or no down-scaling) in the appropriate X/Y[1] registers. Then set the source up-scaling using this ratio: 4096:(set X/Y[0])

For example, if you want your image to be 1:1, then use a down-scale setting of 4096 and an up- scale setting of 4096. If you want your image to be double size, 2:1, then use an up- scale setting of 2048. If you want your image to be 2.32992:1, then use an up- scale setting of 879.

To shrink the destination bitmap, set the up-scale value to 4096. Then set the down- scale value using this ratio: (set X/Y[1]): 4096

If you want your pasted bitmap to be 1:1, then set the down-scale setting to 4096.  
If you want your image to be half size, e.g. 1:2, then use a down-scale setting of 2048.  
If you want your image to be 0.707:1, or, 1:1.41421, then use a down sample setting of 2896 (this value is relevant to 45-degree rotations on blitted bitmaps).

*You may mix different X&Y scale figures including a zoom on one axis and a shrink on the other. Note that the H&V center paste will not work properly with any zoom setting other than 1:1. This is because to obtain the proper center offset based on the source width and height, we need to calculate the reciprocal of the source scale setting to determine the size of the final image which can give us the center offset of that image.  A reciprocal is long division and there is no more space in the current FPGA.*

### Copy Colour Transform (08)

Sets a colour transformation on the blitter copy command. This causes the blitter to XOR read pixels with the Low Byte of this command.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | m | m | m | m | m | m | m | m |

* m – 8-bit colour mask value
* x – don’t care – these bits are ignored

|  |  |  |
| --- | --- | --- |
| **INPUT** | | **OUTPUT** |
| **A** | B | A XOR B |
| 0 | 0 | 0 |
| 0 | 1 | 1 |
| 1 | 0 | 1 |
| 1 | 1 | 0 |

*When using the mask feature the transparent colour is '0x00'. XORing the read pixels with a custom number here other than '0x00' will change the read colour which will simultaneously change what colour will become transparent when a paste/write pixel is done with mask enable.*

The chosen drawing colour, in the Low Byte when the drawing command is sent to the HAG, will perform a second XORing of the first XORed pixel copy, then allow you to change the colour once again before the pixel is written.

So, if the source image is monochrome 1-bit color and the destination screen is 4-bit 16 colours, using a number like 0x04 to XOR the read values, will make the output colour 0x04 and 0x05 instead of 0x00 and 0x01.

Be careful not to choose a XOR number larger than the available colours on the destination screen, otherwise garbage will bleed into adjacent pixels.

### Blitter Function – (00)

Enables the blitter and sets its function according to bits 0-2 of the Low Byte (values 0-7):

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HIGH BYTE | | | | | | | | LOW BYTE | | | | | | | |
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0 |
| 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | x | x | x | x | x | f | f | f |

* f – sets required function – see table below
* x – don’t care – these bits are ignored

|  |  |  |
| --- | --- | --- |
| **Bit** | **Function** | **Details** |
| 0 | Blitter | HIGH – Enables blitter, copying source to output coordinates.  LOW – Blitter disabled, normal pixel write commands. |
| 1 | Paste Mask | HIGH – Pastes pixels with transparency mask.  LOW – Paste pixels even if the source has the selected transparent colour. |
| 2 | Centre Paste | HIGH – Offset the paste up and to the left by half of blit\_width/height  LOW – Use the paste coordinates as the top-left. |

## HAG Bit Plane Values

When setting bits per pixel, or bit plane values for the HAG, do not use the table provided for the MAGGIE settings. Bits per pixel values for the HAG are the desired bpp value minus 1. So, 1 bpp would be a value of 0, 4 bpp would be 3 etc.

# Appendix A – Character Codepage

